Linksys, A division of Cisco Systems, Inc.

Product:                WRT54G

Classification:         Firmware Release History

Firmware  Date:		1/3/2005

Release Date:           1/28/2005

Last Firmware Version: 3.03.6 __________________________________________________________________________
Firmware 3.03.6
- Supports hardware version 3
- Updated help file

Firmware 3.03.1
- Wi-Fi certified

Firmware 3.01.3
- Updated wireless driver
- Supports hardware version 2.2 (cannot downgrade to previous versions)
- Resolves issue with VoIP adapters
- Resolves issue with long domain names

Firmware 2.04.4
- Updated wireless driver
- Updated certificate generation for https access

Firmware 2.04.3
- Resolves issue with disabling firewall
- Added QoS function
- Added Port Triggering function
- Added L2TP option for WAN connection type
- Added ability to back up and restore configuration files
- Added Wireless isolation function
- Added ability to filter internal NAT redirection
- Added ability to restrict access to web GUI from wireless clients
- Added ability to filter IDENT port 113
- Resolves issue with HeartBeat WAN connection
- Added support for 40/56bit cipher to support old browsers to use https
- Resolves issue with PPTP passthrough
- Changed WPA Group Key renewal time range to 600~7200 seconds
- Added IGMP proxy support
- Added ability to allow web GUI access only through https or http


Firmware 2.02.2
- Updated wireless driver to support all versions of WRT54G hardware
- Adds support to allow WAP54G connect as a repeater
- CTS protection mode set to disable by default to improve wireless performance in normal environments
- Resolved issue where the WLAN LED stays on even when wireless is disabled
- Resolved security vulnerability causing the web server in the router to crash

Firmware 2.00.8 (WRT54G v.2 only)
- Updated wireless driver

Firmware Version 1.42.2
- Updated wireless driver to 3.31.15
- Added URL and contents filters
- Added L2TP passthrough
- Added HeartBeat Signal support
- Resolved issue with Connect on Demand

Firmware Version 1.41.2
- Updated GUI format and layout

Firmware Version 1.30.7
- Adds UI control to enable/disable frame bursting
- Resolves issue with firmware upgrade error in Internet Explorer 6.0.2800.1106.xpsp2.030422-1633, on Windows XP pro.
- Send 192.168.1.1 to disable DynDNS
- Resolves issue with using the 4th tx key for WEP
- Resolves issue with disconnecting PPPoE causing WPA to be disabled

Firmware Version 1.30.1
- Adjust PPTP max MTU value from 1400 to 1460 
- The router is now certifiable for the UPnP logo
- Complies with final 802.11g standard
- Improved performance asymmetry between the transmit and receive paths
- Receive Broadcast packets from renew state. Some DHCP server (Dlink 300G+) send broadcast ACK after it receives a REQUEST
- Fix: The firmware upgrade will fail, if DDNS updates while upgrading
- Fix: If first DNS address fails, the second or third DNS address will be used to resolve domain names
- Added the following items under Setup Page:	
    - Router Name
    - Manual Time Server
    - MAC Clone
    - wireless domain
    - Security Settings 
- Added the following items under System Page
    - UPnP enable/disable
    - Ping Test and Traceroute
- Added the following items under Wireless Page
    - CTS Protection Mode
    - Basic Rate
- Added the following items under Status Page
    - Router Name
    - Start IP Address
    - End IP Address
- Added Wi-Fi Protected Access(TM) support including AES and TKIP encryption
- Resolves issue with Port Forwarding name showing up as garbage characters
- Added "B-Only" option to wireless modes
- Added "Default" option to Basic Rate settings

Firmware Version 1.02.1
- Incorporates updates found in the Draft IEEE 802.11g version 6.1 specification
- Resolves interoperability issues with legacy 802.11b devices under Mixed Mode 
- Resolves a performance bug where the performance in a mixed b, g network did not go up once the last b client disassociated
- Resolves issue where WEP degrades performance
- Resolves issue with TZO DDNS Service 
- "Domain Name" replaces "name"
- TFTP server will only verify image file name "xxxx.bin"
- MAC Address Filter under the Advanced tab works on both wired and wireless clients
- Fixed a bug that prevented wireless clients from connecting to the Internet if there was no active wired PC (PPoE customers in Europe and China only)
- Support for UPnP enabled applications such as MSN Messenger
- Fixed a bug that caused computers connected to the LAN ports to be dropped at some interval only to be immediately re-connected
- Fixed Dynamic Routing issue between 2 Routers
- Allows User to name Static Route Configurations
- Modified PC List Web Page to avoid confusion
- Stabilized Wireless-G to LAN and WAN Throughput
- Stabilized Wireless-B to LAN and WAN Throughput
- Improved LAN-WAN Throughput

Firmware Ver.:	1.01
- Initial release